**24**

**VT**

**ISOLATOR**

**493**

**OPEN**

**13**

**BCU**

**ABNORMAL**

**23**

**VT 493**

**ISOLATOR**

**SWITCHING**

**INCOMPLETE**

**12**

**COMP.(G04-5)**

**GAS DENSITY**

**HIGH**

**11**

**COMP.(G04-5)**

**GAS PRESSURE**

**LOW STAGE 1**

**22**

**GIS VT-L6**

**AUX. MCB**

**TRIPPED**

**21**

**GIS VT-L6**

**MAIN MCB**

**TRIPPED**

**22**

**GIS VT-L4**

**AUX. MCB**

**TRRIPED**

**21**

**GIS VT-L4**

**MAIN MCB**

**TRIPPED**

**10**

**COMP.(G04-3)**

**GAS DENSITY**

**HIGH**

**9**

**COMP.(G04-4)**

**GAS PRESSURE**

**LOW STAGE 1**

**4**

**COMP.(G04-2)**

**GAS PRESSURE**

**LOW STAGE 1**

**3**

**COMP.(G04-1)**

**GAS DENSITY**

**HIGH**

**28**

**ANN.**

**DC POWER**

**FAILURE**

**26**

**32**

**BCU FAULTY**

**/INTERNAL**

**FAILURE**

**31**

**20**

**BCU**

**ABNORMAL**

**17**

**SPRING**

**CHARGE MOTOR EXCESSIVE RUNNING**

**19**

**SPRING**

**CHARGE MOTOR**

**LOCKED OUT**

**8**

**30**

**29**

**18**

**SPRING**

**CHARGE MOTOR THERMAL**

**FAULT**

**7**

**COMP.(G04-3)**

**GAS DENSITY**

**HIGH**

**14**

**COMP.(G04-1)**

**GAS DENSITY**

**HIGH**

**6**

**COMP.(G04-3)**

**GAS PRESSURE**

**LOW STAGE 1**

**5**

**COMP.(G04-2)**

**GAS DENSITY**

**HIGH**

**27**

**ANN.**

**AC POWER**

**FAILURE**

**16**

**15**

**25**

**13**

**COMP.(G04-6)**

**GAS PRESSURE**

**LOW STAGE 1**

**2**

**COMP.(G04-1)**

**GAS PRESSURE**

**LOW STAGE 1**

**1**

**CB. COMP.(G04-0)**

**GAS DENSITY**

**HIGH**