|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GENERAL DATA AND INFORMATION:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LOCATION |  |  | MANUFACTURER | ***Bowthorpe EMP*** |
| PHASE | B – Phase  |  | MODEL no. | SC13 |
| COUNTER SCALE | 0 - 50 mA |  |  |  |

2. MECHANICAL CHECKS AND VISUAL INSPECTION:

|  |  |  |
| --- | --- | --- |
| ITEM | DESCRIPTION | CHECKED |
| 1 | Inspect for any physical damage or defects. |  |
| 2 | Verify nameplate information for correctness |  |
| 3 | Check tightness of all bolted connections. |  |

3. ELECTRICAL TESTS:

|  |  |  |  |
| --- | --- | --- | --- |
| COUNTER SCALE | MEASURED VALUES | ERROR % | REMARKS |
| 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| 10 |  |  |  |
| 30 |  |  |  |
| 50 |  |  |  |

 |